



Eco Backrest Assembly:

Eco Backrest Assembly:

1-- Place the cushion on a bed or floor with the straps unbuckled. If the cushion has a removable cover, that should be in place first.



1-- Place the cushion on a bed or floor with the straps unbuckled. If the cushion has a removable cover, that should be in place first.

2-- Remove the Velcro loop and place the wooden seat on top of the cushion hinge side up. The back support board should be lined up with the back cushion and the base should be lined up with the floor cushion.

2-- Remove the Velcro loop and place the wooden seat on top of the cushion hinge side up. The back support board should be lined up with the back cushion and the
base should be lined up with the floor cushion.



3-- Attach the cushion to the back support board by inserting each end
of each strap through the matching holes. There are four pairs of holes.

with the floor cushion.

3-- Attach the cushion to the back support board by inserting each end
of each strap through the matching holes. There are four pairs of holes.

with the floor cushion.

4-- The tension strap should come already threaded. If it comes
unthreaded, you can rethread it using the two parallel slots on the
back support board and the angle board. With the Tension Strap
unclipped, thread the female side through the back support board, and
the male side though the angle board with the open-end/tail facing up.

4-- The tension strap should come already threaded. If it comes
unthreaded, simply rethread it using the two parallel slots on the
back support board and the angle board. With the Tension Strap
unclipped, thread the female side through the back support board, and the male side though the angle board with the open-end/tail facing up.





Backrest storage / travel:

The eco backrest is designed to be easily moved and stored.
1-- To move or store the backrest, first open the Velcro storage loop.

6-- Clip the tension strap and tighten it by holding the buckle and
pulling the open-end/ tail.
The eco backrest is now set up and ready to use. NOTE: the tension
strap is a safety feature. Only sit in the eco backrest when it is
engaged. As long as the tension strap is buckled and taut, the eco back rest can be easy moved.

6-- Clip the tension strap and tighten it by holding the buckle and
pulling the open-end/ tail.
The eco backrest is now set up and ready to use. NOTE: the tension
strap is a safety feature. Only sit in the eco backrest when it is
engaged. As long as the tension strap is buckled and taut, it can be
easy moved.

2-- Unclip the tension strap. Then, with one hand on back support board and one hand on the angle board, un-slot the angle board from the back support board and bring the handles together.
4-- Finally, tightly wrap the Velcro storage loop around the handles
of both the back support board and the angle board. You may have to
push the tension strap out of the way in order to do this.

2-- Unclip the tension strap. Then, with one hand on back support board and one hand on the angle board, un-slot the angle board from the back support board and bring the handles together.
4-- Finally, tightly wrap the Velcro storage loop around the handles
of both the back support board and the angle board. You may have to
push the tension strap out of the way in order to do this.

Backrest storage / travel:
The eco backrest is designed to be easily moved and stored.
1-- To move or store the backrest, first open the velcro storage loop.

5-- Choose a setting and make sure the tension strap is unbuckled with
plenty of slack. Then slot the angle board into one of the three slots
in the back support board.

5-- Choose a setting and make sure the tension strap is unbuckled with
plenty of slack. Then slot the angle board into one of the three slots
in the back support board.